{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["CDKOHSL","说明","工程量清单"],"not_rendered":{"defined_names":4},"read":"whole","date_system":"1900"}

{"sheet":"CDKOHSL","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true}

{"sheet":"说明","index":1,"n_rows":9,"n_cols":1,"rows_kept":9}
["工程量清单说明"]
["        1. 招标清单中所列工程数量是估算或设计的预计数量，仅作为投标的共同基础，除有另行规定外不能作为最终结算与支付的依据。实际支付应按经甲方确认的实际完成工程量进行计量结算。\n"]
["        2. 合同单价为固定综合单价，正常情况下不作调整。综合单价中已经包含为实施和完成合同工程所需的劳务费、材料费（甲方提供材料除外）、机械、质检（自检）、安装费、缺陷修复、措施费、管理费、规费、施工辅助费、保险、利润、水电费、所有材料设备装卸运输费、二次倒运费、小型临时设施费用、冬雨季及夜间施工措施费、进出场费、工程检测试验费用、迎检费用、标准化施工费、已完工程及设备保护费、场地清理费、各种培训费用、除增值税以外的其他税金，地方收取的各种费用等以及为完成该项工程协议明示或暗示的所有责任、义务和一切风险的费用。\n"]
["        3. 施工内容包含但不限于施工交验合格的成品、施工后现场整形及养护、成品保护、施工质量检验所要求的检测、取样、试验、测量、资料编制等内容，图纸、技术规范、施工现场及图集规范要求的全部相关工作内容，以及其他为完成本招标工程施工范围所应承担的工作。\n"]
["        4. 本项目投标报价合价金额不含安全文明施工费。安全文明施工费依据承包人每月结算金额（不含税）的2%另行支付。\n"]
["        5. 本项目投标报价合价金额不含增值税税额。增值税依据承包人实际开具的增值税发票票面税额另行支付。\n"]
["        6. 本清单各子目“投标报价单价（不含税）”由投标人自行填报，且不得超过最高限价单价（不含税），每个清单子目，必须填入单价。"]
["        7. 各项目详细做法根据图纸及现场情况自行考虑。\n"]
["        8. 清单未尽事宜由招标方另行解释。\n"]

{"sheet":"工程量清单","index":2,"n_rows":69,"n_cols":13,"rows_kept":69,"merged":[[0,0,0,9],[1,3,1,6],[68,0,68,7]]}
["哈素海服务区劳务招标项目清单"]
["标段编号：哈素海服务区",{"$nulls":8},"货币单位：人民币元"]
["序号","项目名称","定额详述","单位","工程量","承包方式","最高限价单价\n（不含税）","投标报价单价\n（不含税）","投标报价合价\n（不含税）","备注"]
[1,"一、防水工程",{"$nulls":6},{"$f":"IF(H4>G4,\"报价无效\",H4*E4)","v":{"v":0,"d":"0.00"}}]
[2,"屋面防水找平层","20厚1：2.5水泥砂浆找平层。","m2",924,"包工包料",22.94,null,{"$f":"IF(H5>G5,\"报价无效\",H5*E5)","v":{"v":0,"d":"0.00"}}]
[3,"屋面防水卷材","3+4SBS防水卷材（不带岩片）\n涂刷两遍冷底油","m2",2115,"包工包料",{"v":105.5,"d":"105.50"},null,{"v":0,"d":"0.00"}]
[4,"二、天棚工程",{"$nulls":4},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
[5,"吊顶天棚-矿棉板","1.吊顶形式、吊杆规格、高度:不上人\n2.龙骨材料种类、规格、中距:U型轻钢龙骨\n3.面层材料品种、规格:600*600mm矿棉板\n4.压条材料种类、规格:矿棉板收口条","m2",181.44,"包工包料",73.39,null,{"v":0,"d":"0.00"}]
[6,"吊顶天棚-铝扣板","1.吊顶形式、吊杆规格、高度:不上人\n2.龙骨材料种类、规格、中距:U型轻钢龙骨\n3.面层材料品种、规格:300*300mm铝扣板\n4.压条材料种类、规格:收口条","m2",1010.61,"包工包料",119.27,null,{"v":0,"d":"0.00"}]
[7,"三、涂料工程",{"$nulls":4},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
[8,"墙面一般抹灰","1.底层厚度、砂浆配合比:1:2.5水泥砂浆抹灰","m2",36,"包工包料",32.11,null,{"v":0,"d":"0.00"}]
[9,"内墙面喷刷涂料","1.刮腻子要求:2厚面层耐水腻子分遍刮平\n2.涂料品种、喷刷遍数:乳胶漆饰面，底漆一遍，面漆一遍。","m2",2277.2,"包工包料",27.52,null,{"$f":"IF(H12>G12,\"报价无效\",H12*E12)","v":{"v":0,"d":"0.00"}},{"$nulls":3}," "]
[10,"四、外墙工程",{"$nulls":4},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
[11,"保温","50mm厚挤塑聚苯板保温层，配套胶粘剂黏粘，辅锚栓固定,三灰两网（容重≥30kg/m3,品牌符合要求）","m2",64.16,"包工包料",110.09,null,{"v":0,"d":"0.00"}]
[12,"外墙面真石漆涂料\n（新做）","\n1.刮腻子要求:配套基层饰面按厂家要求，二遍外墙腻子\n2.涂料品种、喷刷遍数:真石漆主层涂料，真石漆面层涂料两遍","m2",800,"包工包料",91.74,null,{"v":0,"d":"0.00"}]
[13,"外墙面涂料\n（在原基层做）\n\n\n","1.基层清理，刷界面剂一道（保温锚栓加固）\n2.腻子种类:5厚聚合物抗裂砂浆复合耐碱网布找平（应达到聚合物防水砂浆性能指标要求，兼做防水保护层）\n3.刮腻子要求:配套基层饰面按厂家要求，二遍外墙腻子\n4.涂料品种、喷刷遍数:真石漆主层涂料，真石漆面层涂料两遍","m2",3109.12,"包工包料",110.09,null,{"v":0,"d":"0.00"}]
[14,"外墙蘑菇砖粘贴","1.基层清理，刷界面剂一道\n2.用瓷砖粘接剂粘贴外墙瓷砖\n3.瓷砖勾缝\n4.瓷砖清洗\n","m2",79,"包工包料",110.09,null,{"v":0,"d":"0.00"}]
[15,"宿舍楼外墙涂料","1.刮腻子要求:配套基层饰面按厂家要求，二遍外墙腻子\n2.涂料品种、喷刷遍数:外墙主层涂料，外墙面层涂料两遍","m2",1845.48,"包工包料",45.87,null,{"v":0,"d":"0.00"}]
[16,"六、隔断类",{"$nulls":4},{"v":0,"d":"0.00"},null,{"$f":"IF(H19>G19,\"报价无效\",H19*E19)","v":{"v":0,"d":"0.00"}}]
[17,"100mm轻钢龙骨隔墙","1.骨架、边框材料种类、规格:100mm轻钢龙骨隔墙\n2.隔板材料品种、规格、颜色:双面石膏板面层，内塞100mm保温岩棉板\n（容重120-140kg/m3,品牌符合要求）","m2",67.2,"包工包料",165.14,null,{"$f":"IF(H20>G20,\"报价无效\",H20*E20)","v":{"v":0,"d":"0.00"}}]
[18,"七、卫生间配件",{"$nulls":4},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
[19,"洗漱台","1.1.5#热镀锌支架\n2.人造石洗面台（包括结晶、磨边、台面开孔及倒角）","m2",40.32,"包工包料",596.33,null,{"v":0,"d":"0.00"}]
[20,"洗漱柜","1.成品洗漱柜（暂按800mm高）","m2",32.75,"包工包料",1055.05,null,{"v":0,"d":"0.00"}]
[21,"成品隔断","1.成品厕浴隔断","m2",224,"包工包料",183.49,null,{"v":0,"d":"0.00"}]
[22,"砌筑蹲位地台","1.新砌筑蹲位，红砖砌筑及水泥砂浆抹灰\n2.地台：高150（不含瓷砖）","m3",29.54,"包工包料",{"v":642.2,"d":"642.20"},null,{"v":0,"d":"0.00"}]
[23,"银镜","1.5mm银镜","m2",87.08,"包工包料",183.49,null,{"v":0,"d":"0.00"}]
[24,"九、安装工程",{"$nulls":4},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
[25,"排水管","1.规格、压力等级:DN110，PVC管","m",215,"包工包料",55.05,null,{"v":0,"d":"0.00"}]
[26,"铸铁散热器","1.铸铁片头柱式散热器（20片）","组",30,"包工包料",981.65,null,{"$f":"IF(H29>G29,\"报价无效\",H29*E29)","v":{"v":0,"d":"0.00"}}]
[27,"地漏","1. 安装地漏（品牌符合甲方要求）","个",37,"包工包料",91.74,null,{"$f":"IF(H30>G30,\"报价无效\",H30*E30)","v":{"v":0,"d":"0.00"}}]
[28,"配管","JDG20","米",84,"包工包料",16.51,null,{"v":0,"d":"0.00"}]
[29,"配线","1.名称:管内或桥架穿线\n2.配线形式:照明线路\n3.型号:国标WDZB-BYJ\n4.规格:2.5\n5.材质:铜芯\n6.配线部位:暗敷","m",306.5,"包工包料",{"v":5.5,"d":"5.50"},null,{"v":0,"d":"0.00"}]
[30,"配线","1.名称:管内或桥架穿线\n2.配线形式:照明线路\n3.型号:国标WDZB-BYJ\n4.规格:4\n5.材质:铜芯\n6.配线部位:暗敷","m",694.5,"包工包料",6.42,null,{"v":0,"d":"0.00"}]
[31,"照明开关","1. 名称: 密闭型单联单控开关（安全型、防水型、IP54）（品牌符合甲方要求）\n2. 规格: 250V 10A\n3.满足相关规范及甲方要求","个",35,"包工包料",18.35,null,{"v":0,"d":"0.00"}]
[32,"照明开关","单相二三眼安全型插座","个",68,"包工包料",20.18,null,{"v":0,"d":"0.00"}]
[33,"照明开关","双联控暗开关（防溅）","个",2,"包工包料",32.11,null,{"v":0,"d":"0.00"}]
[34,"LED平板灯","  1*18W","套",62,"包工包料",82.57,null,{"v":0,"d":"0.00"}]
[35,"墙面开槽","施工满足规范要求","m",59.5,"包工包料",11.01,null,{"v":0,"d":"0.00"}]
[36,"十四、其它工程",{"$nulls":4},{"v":0,"d":"0.00"},null,{"$f":"IF(H39>G39,\"报价无效\",H39*E39)","v":{"v":0,"d":"0.00"}}]
[37,"砌块墙","1.砌块品种、规格、强度等级:200*200*600蒸压加气块墙体","m3",12.46,"包工包料",458.72,null,{"$f":"IF(H40>G40,\"报价无效\",H40*E40)","v":{"v":0,"d":"0.00"}}]
[38,"路缘石","1.600*150*50路缘石安装（不含路缘石材料）\n2.1:3水泥砂浆结合层\n3.C20混凝土靠背施工\n4.路缘石之间缝隙勾缝","m",460,"包工包料",45.87,null,{"v":0,"d":"0.00"}]
[39,"透水砖","1.60厚1:3干硬性水泥砂浆\n2.250*125*60厚块料砖铺实拍平，稀水泥浆擦缝","平米",1093.44,"重包",100.92,null,{"$f":"IF(H42>G42,\"报价无效\",H42*E42)","v":{"v":0,"d":"0.00"}}]
[40,"植草砖","1.60厚1:3干硬性水泥砂浆\n2.250*125*60厚块料砖铺实拍平，稀水泥浆擦缝","平米",3856.88,"重包",100.92,null,{"v":0,"d":"0.00"}]
[41,"踢脚线","1.面砖踢脚线粘接\n2.10mm厚1:3水泥砂浆压实抹\n平\n3.3mm厚外加剂专用砂浆抹基\n底刮糙\n4.水泥钉固定踢脚上端，中距\n300","米",158.4,"重包",27.52,null,{"v":0,"d":"0.00"}]
[42,"地暖","1、20mm挤塑板\n2、地暖隔热膜\n3、3mm钢丝网片\n4、20mm地暖管\n5、50mm厚混凝土保护层\n6、分集水器\n7、打压、试压","平米",766.34,"重包",137.61,null,{"v":0,"d":"0.00"}]
[43,"十五、拆除工程（含垃圾外运）",{"$nulls":4},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
[44,"拆除勒脚","1.名称：拆除勒脚","m2",79,"轻包",14.68,null,{"v":0,"d":"0.00"}]
[45,"防水层拆除","1.名称：拆除屋面防水层","m2",924,"轻包",2.29,null,{"v":0,"d":"0.00"}]
[46,"拆除厕浴隔断","1.名称：厕浴隔断拆除","套",224,"轻包",7.34,null,{"v":0,"d":"0.00"}]
[47,"拆除底柜","1.名称：洗漱柜拆除","m2",32.75,"轻包",16.51,null,{"v":0,"d":"0.00"}]
[48,"铲除涂料面-内墙、顶面","1.名称：铲除内墙涂料","m2",2277.2,"轻包",2.75,null,{"v":0,"d":"0.00"}]
[49,"立面块料拆除","1.名称：墙砖拆除，包含抹灰层","m2",1978.14,"轻包",14.68,null,{"v":0,"d":"0.00"}]
[50,"木门窗拆除","1.拆除门窗洞口尺寸：木质门（1000*2100）","樘",10,"轻包",39.45,null,{"$f":"IF(H53>G53,\"报价无效\",H53*E53)","v":{"v":0,"d":"0.00"}}]
[51,"平面块料拆除","1.拆除地砖，包含垫层\n","m2",1450.6,"轻包",41.28,null,{"v":0,"d":"0.00"}]
[52,"天棚面龙骨及饰面拆除","1.名称：矿棉板/PVC吊顶龙骨及面层拆除","m2",1168.18,"轻包",7.34,null,{"v":0,"d":"0.00"}]
[53,"洗漱台拆除","1.名称：洗手池台面拆除","m2",40.32,"轻包",20.18,null,{"v":0,"d":"0.00"}]
[54,"外墙保温","1.拆除原有外墙保温。","m2",64.16,"轻包",20.18,null,{"v":0,"d":"0.00"}]
[55,"铲除涂料面-外墙","1.名称：铲除外墙涂料","m2",81.8,"轻包",2.75,null,{"$f":"IF(H58>G58,\"报价无效\",H58*E58)","v":{"v":0,"d":"0.00"}}]
[56,"拆除蹲便器","1.名称：蹲便器拆除","套",186,"轻包",45.87,null,{"v":0,"d":"0.00"}]
[57,"拆除洗脸池","1.名称：面池拆除","套",80,"轻包",27.52,null,{"v":0,"d":"0.00"}]
[58,"拆除小便器","1.名称：小便器拆除","套",48,"轻包",27.52,null,{"v":0,"d":"0.00"}]
[59,"管道拆除","1.拆除原有雨水立管DN110PVC、支管等","m",215,"轻包",9.17,null,{"v":0,"d":"0.00"}]
[60,"暖气片拆除","1.拆除暖气片\n","组",30,"轻包",32.11,null,{"v":0,"d":"0.00"}]
[61,"拆除原有路缘石",null,"米",460,"轻包",6.42,null,{"v":0,"d":"0.00"}]
[62,"拆除南北广场面包砖",null,"m2",5352.2,"轻包",11.93,null,{"v":0,"d":"0.00"}]
[63,"拆除地梁",null,"m",17.8,"轻包",513.76,null,{"v":0,"d":"0.00"}]
[64,"屋面防水拆除","1.拆除防水层               \n2.女儿墙底部0.8m高范围内保温层拆除\n3.伸缩缝镀锌铁皮盖板拆除","m2",924,"轻包",10.09,null,{"v":0,"d":"0.00"}]
[65,"垃圾外运","拆除工程、施工过程中产生的垃圾机械装车、外运、运距自行考虑","m3",1,null,137.61,null,{"v":0,"d":"0.00"}]
["投标报价总计",{"$nulls":7},{"$f":"SUM(I4:I68)","v":{"v":0,"d":"0.00"}}]